Measurement type

Range

Range AC : 0 -500 V

DC : 48 V

Ohms : 1 ohm- 1M ohm

Select the type of measurement - Voltage

Current

Ohms

Unit

Result of measurement calculations

Attenuator/ Amplifier

ADC

Filters

Data serializer

Output to Socket

Data from front end

to UI program

Input from Socket

Data deserializer

Measurement calculations

Input signal conditioning block

Display

Source